
Technical data

(Models with standard wheelbase 2980 mm, W 251 series)

	R 300 CDI BlueEFFICIENCY



	Engine and performance
	

	Cylinder arrangement/number 
	V6

	Displacement (cc) 
	2 987

	Rated output (kW at r/min) 1) 
	140 /3 800

	Rated torque (Nm at r/min) 2) 
	440/1 400 – 2 800

	Compression ratio 
	15.5 : 1

	Acceleration 0-100 km/h (sec) 
	9.5

	Maximum speed (km/h) 
	215

	Power transmission
	

	Drive system 
	Rear-wheel drive

	Transmission 
	7G-TRONIC

	Ratios 
	4.38/2.86/1.92/1.37/1.00/0.82/0.73/

Rev 3.416

	Final drive ratio 
	2.920

	Fuel, emissions & insurance category
	

	Tank capacity/incl. reserve (l) 
	80/13.0

	Fuel consumption urban (l/100 km) 3) 
	9.6-9.9

	Fuel consumption extra-urban (l/100 km) 3) 
	6.4-6.7

	Fuel consumption combined (l/100 km) 3) 
	7.6 - 7.8

	CO2 emissions combined (g/km) 3) 
	199 - 206

	Cd figure 
	0.31

	Emissions class 
	Euro 5

	Insurance category 3rd party/fully-comp./semi-comp. 
	23/29/27

	Suspension & steering
	

	Front axle 
	Double wishbone

	Rear axle 
	Multi-link

	Springs front / rear 
	Coil springs, single-tube gas-pressure/ coil springs, single-tube gas-pressure

	Tyres/wheels front 
	255/55 R 18

	Tyres/wheels rear 
	255/55 R 18

	Steering 
	Rack-and-pinion steering, hydraulic

	Front brakes 
	Disc brakes, internally ventilated

	Rear brakes 
	Disc brakes

	Dimensions and weights
	

	Kerb weight/payload (kg) 4) 
	2 185/655

	Permissible gross vehicle weight (kg) 
	2 840

	Maximum roof load (kg) 
	100

	Luggage capacity (VDA) min/max (l) 
	550/1 950

	Perm. trailer load unbraked/braked (kg) 
	750/2 100

	Perm. drawbar load (kg) 
	85

	Turning circle (m) 
	11.8

	Overall length (mm) 
	4 922

	Overall width (mm) 
	1 922

	Overall height at kerb weight (mm) 
	1 674

	Track, front (mm) 
	1 661

	Track, rear (mm) 
	1 651

	Wheelbase (mm) 
	2 980


	R 300



	Engine and performance  

	Cylinder arrangement/number 
	V6 

	Displacement (cc) 
	2 996 

	Rated output (kW  at r/min)1 
	170 /6 000 

	Rated torque (Nm at r/min)2 
	300/2 500 – 5 000 

	Compression ratio 
	11.3 : 1 

	Acceleration 0-100 km/h (sec) 
	9.6 

	Maximum speed (km/h) 
	222 

	Power transmission

	Drive system 
	Rear-wheel drive 

	Transmission 
	7G-TRONIC 

	Ratios 
	4.38/2.86/1.92/1.37/1.00/0.82/0.73/
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	Final drive ratio 
	3 900 

	Fuel, emissions & insurance category

	Tank capacity/incl. reserve (l) 
	80/13.0 

	Fuel consumption urban (l/100 km)3 
	15.2-15.4 

	Fuel consumption extra-urban (l/100 km)3 
	8.8-9.0 

	Fuel consumption combined (l/100 km)3 
	11.1 - 11.3 

	CO2 emissions combined (g/km)3 
	260-265 

	Cd figure 
	0.32 

	Emissions class 
	Euro 5 

	Insurance category 3rd party/fully-comp./semi-comp. 
	21/28/27 

	Suspension & steering 

	Front axle 
	Double wishbone 

	Rear axle 
	Multi-link 

	Springs front / rear 
	Coil springs, single-tube gas-pressure/ coil springs, single-tube gas-pressure 

	Tyres/wheels front 
	255/55 R 18 

	Tyres/wheels rear 
	255/55 R 18 

	Steering 
	Speed-sensitive rack-and-pinion steering, hydraulic 

	Front brakes 
	Disc brakes, internally ventilated 

	Rear brakes 
	Disc brakes 


	Dimensions and weights 

	Kerb weight/payload (kg)4 
	2 130/660 

	Permissible gross vehicle weight (kg) 
	2 790 

	Maximum roof load (kg) 
	100 

	Luggage capacity (VDA) min/max (l) 
	550/1 950 

	Perm. trailer load unbraked/braked (kg) 
	750/2 100 

	Perm. drawbar load (kg) 
	85 

	Turning circle (m) 
	11.80 

	Overall length (mm) 
	4 922 

	Overall width (mm) 
	1 922 

	Overall height at kerb weight (mm) 
	1 676 

	Track, front (mm) 
	1 639 

	Track, rear (mm) 
	1 629 

	Wheelbase (mm) 
	2 980 


	R 500 4MATIC



	Engine and performance

	Cylinder arrangement/number 
	V8 

	Displacement (cc) 
	5 461 

	Rated output (kW  at r/min)1 
	285 [388]/6 000 

	Rated torque (Nm at r/min)2 
	530/2 800–4 800 

	Compression ratio 
	10.7 : 1 

	Acceleration 0-100 km/h (sec) 
	6.3 

	Maximum speed (km/h) 
	250 

	Power transmission 

	Drive system 
	Permanent all-wheel drive 

	Transmission 
	7G-TRONIC 

	Ratios 
	4.38/2.86/1.92/1.37/1.00/0.82/0.73/
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	Final drive ratio 
	3.45 

	Fuel, emissions & insurance category 

	Tank capacity/incl. reserve (l) 
	80/13.0 

	Fuel consumption urban (l/100 km)3 
	18.6-18.8 

	Fuel consumption extra-urban (l/100 km)3 
	10.0 - 10.2 

	Fuel consumption combined (l/100 km)3 
	13.2 - 13.4 

	CO2 emissions combined (g/km)3 
	306 - 311 

	Cd figure 
	0.32 

	Emissions class 
	Euro 5 

	Insurance category 3rd party/fully-comp./semi-comp. 
	21/28/27 

	Suspension & steering 

	Front axle 
	Double wishbone 

	Rear axle 
	Multi-link 

	Springs front / rear 
	Coil spring, single-tube gas-pressure/ air spring, single-tube gas-pressure 

	Tyres/wheels front 
	255/50 R 19 

	Tyres/wheels rear 
	255/50 R 19 

	Steering 
	Speed-sensitive rack-and-pinion steering, hydraulic 

	Front brakes 
	Disc brakes, internally ventilated 

	Rear brakes 
	Disc brakes, internally ventilated 


	Dimensions and weights

	Kerb weight/payload (kg)4 
	2 265/655 

	Permissible gross vehicle weight (kg) 
	2 920 

	Maximum roof load (kg) 
	100 

	Luggage capacity (VDA) min/max (l) 
	633/2 385 

	Perm. trailer load unbraked/braked (kg) 
	750/2 100 

	Perm. drawbar load (kg) 
	85 

	Turning circle (m) 
	12.60 

	Overall length (mm) 
	5 157 

	Overall width (mm) 
	1 922 

	Overall height at kerb weight (mm) 
	1 666 

	Track, front (mm) 
	1 638 

	Track, rear (mm) 
	1 636 

	Wheelbase (mm) 
	3 215 


1) Rated output figures according to Directive 80/1269/EEC in the version valid at the time.

2) Rated torque figures according to Directive 80/1269/EEC in the version valid at the time.

3) Figures established according to the measuring methods prescribed by Directive 80/1268/EEC in the version valid at the time. The figures do not refer to any individual vehicle and do not constitute part of an offer, but are merely for the purposes of comparison between the different vehicle models.

4) Figures are in accordance with Directive 92/21/EC, version 95/48/EC (mass in ready-to-drive condition, fuel tank 90 % full, with driver weighing 68 kg and luggage 7 kg) for vehicles with standard equipment. Optional extras and accessories usually increase this figure, with a corresponding reduction in payload.
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