2011 FREELANDER 2 TECHNICAL DATA

	
	TD4 110kW Manual 4WD
	SD4 140kW Auto 4WD

	Height mm
	1740
	1740

	Width mm
	2195
	2195

	Length mm
	4500
	4500

	Wheelbase mm
	2660
	2660

	Turning Circle m
	11.3
	11.3

	Min Weight from kg
	1785
	1805

	Front suspension
	Macpherson strut with lower control arm and anti-roll bar
	Macpherson strut with lower control arm and anti-roll bar

	Rear suspension
	Strut assembly with lateral and longitudinal links and anti-roll bar
	Strut assembly with lateral and longitudinal links and anti-roll bar

	Brakes Front
	Ventilated front disc -  300mm, solid rear – 302mm
	Ventilated front disc -  300mm, solid rear – 302mm

	Steering
	Hydraulic power assisted rack and pinion
	Hydraulic power assisted rack and pinion

	Four Wheel-Drive system
	Full time 4 wheel drive with Haldex rear axle differential.
	Full time 4 wheel drive with Haldex rear axle differential.

	Engine type
	Transverse, in-line 4-cylinder, 16-valve turbo diesel, common rail fuel injection
	Transverse, in-line 4cylinder, 16-valve turbo diesel, common rail fuel injection

	Displacement cc
	2179cc
	2179

	Bore/stroke mm 
	85x96
	85x96

	Compression ratio
	15.8:1
	15.8:1

	Max power kW
	110
	140

	Max Torque Nm 
	420 
	420 

	Fuel consumption EU urban/extra urban/combined (L/100km)
	7.9/5.8/6.6
	8.7/5.7/7.0

	Emissions
	EU4
	EU4

	CO2 g/km
	174
	185

	Transmission
	M66 EH50 6-speed manual
	Aisin SWF21 6 Speed auto

	Fuel tank capacity litres
	68
	68

	0-100 kph
	11.7
	9.5

	Top speed (kph)
	181
	190

	Price (incl. VAT)
	R384 995
	R489 995


