Specifications/Technical data  

	 
	1.4 TB  

88 kW 

Start&Stop
	1.4 TB  

125 kW MultiAir

Start&Stop
	1.750 TBi 

173kW

	DIMENSIONS


	 
	 
	 

	Number of seats
	5
	5
	5

	Number of doors
	5
	5
	5

	length/width (mm)
	4351/1798
	4351/1798
	4351/1798

	height (mm)
	1465
	1465
	1465

	Wheelbase (mm)
	2634
	2634
	2634

	Front/rear track (mm)
	1554/1554
	1554/1554
	1554/1554

	Luggage compartment capacity (dm³)
	350
	350
	350

	ENGINE

 
	 
	 
	 

	Number of cylinders, layout
	4
	4
	4

	Bore and stroke (mm)
	72x84
	72x84
	83x80.5

	Displacement (cc)
	1368
	1368
	1742

	Compression ratio 
	9,8:1
	9,8:1
	9,25:1

	Maximum power output kW (HP - EC) at rpm
	88 at 5,000 revs
	125 at 5,500 revs
	173 at 5,500 revs

	Peak torque Nm (kgm-EC) at rpm (NORMAL)
	206 (21) at 1,750 revs
	230 (23.4) at 2,250 revs
	300 (30.5) at 4,500 revs

	Peak torque Nm (kgm-EC) at rpm (DYNAMIC)
	
	250 (25.4) at 2,500 revs
	340 (34.6) at 1,900 revs

	Distribution (control)
	Toothed belt with hydraulic tappets with fixed timing 
	Toothed belt with hydraulic tappets and intake side Multiair system
	Two continuously variable valve timing units and toothed belt with hydraulic tappets 

	Fuel supply
	MPFI supercharged through exhaust gas turbocharger with intercooler
	MPFI supercharged and MultiAir direct valve control system, intercooler
	Direct petrol injection and turbocharging with scavenging system and intercooler

	Stop&Start system for automatic engine stopping/starting for short stops during city driving, useful for optimising fuel consumption and CO2 emissions
	Standard
	Standard
	N/A

	ELECTRIC EQUIPMENT


	
	
	

	Battery: capacity (Ah) / Generator (A)
	63Ah/450
	63Ah/450
	60Ah/540

	TRANSMISSION 


	
	
	

	Traction
	front
	front
	front

	Gearbox
	6-speed manual
	6-speed manual
	6-speed manual

	First
	1:3,9000
	1:3,9000
	1:3,9000

	Second
	1:2,118
	1:2,118
	1:2,118

	Third
	1:1,484
	1:1,484
	1:1,484

	Fourth
	1:1,116
	1:1,116
	1:1,116

	Fifth
	1:0,897
	1:0,897
	1:0,897

	Sixth
	1:0,767
	1:0,767
	1:0,767

	Reverse
	1:4,000
	1:4,000
	1:4,000

	Final drive torque
	1:4,118
	1:3,833
	1:3,579

	TYRES


	
	
	

	Tyre size
	205/55 R16 91V
	205/55 R16 91V
	225/45 R17 91W

	Rim size
	7J x 16 
	7J x 16 
	7.5J x 17

	STEERING


	
	
	

	Steering box
	Dual Pinion
	Dual Pinion
	Dual Pinion

	Turning circle (m)
	10,9
	10,9
	10,9

	SUSPENSION


	
	
	

	Front

	Rear

	BRAKES D (DISC)


	
	
	

	Front (mm)
	281
	305
	330

	Rear (mm)
	264
	264
	278

	CAPACITIES – WEIGHTS


	
	
	

	Fuel tank (litres)
	60
	60
	60

	Kerb weight (kg)
	1355
	1365
	1395

	Max towing weight (kg) non-braked
	500
	500
	500

	Max towing weight (kg) braked
	1300
	1300
	1300

	Total admissible weight (5 people+ 50 kg load)
	1785
	1795
	1825

	PERFORMANCE


	
	
	

	Max. speed (km/h)
	195
	218
	242

	Acceleration (1 person + 30 kg) 0-100 km/h (s)
	9,4
	7,8
	6,8

	FUEL CONSUMPTION-EMISSIONS as per directive 1999/100/EC        

                               
	
	
	

	Urban cycle fuel consumption (l/100km)
	8,4
	7,8
	10,8

	Extra-urban cycle
	5,3
	4,6
	5,8

	Combined cycle
	6,4
	5,8
	7,6

	CO2 emissions (g/km)
	149
	134
	177

	Service
	30,000 km
	30,000 km
	35,000 km

	Environmental classification
	Euro 5 
	Euro 5 
	Euro 5 

	Pick-up in 5th gear from 60 to 100 km/h
	8,2
	7,3
	6,9

	Pick-up in 6th gear from 80 to 120 km/h
	11,0
	9,3
	8,3


